Custom Design LCM
	Module Structure 

	[image: image1.png]


□COB
	[image: image2.png]mo>

4

ng ,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,

L T




□COG
	□TAB

[image: image3.png]o [ IC | e

iComponenTsoreo:







	Dimensions

	Module Outline：(A)        X (B)        mm

	Viewing Area：(C)      X (D)        mm

	Active Area：(E)      X (F)        mm

	Distance between mounting holes：(G)        X (H)        mm

	Diameter of mounting holes：(M)        mm

	Total thickness：(H1)        mm

	Upper thickness：(H2)        mm

	Display Contents

	□Segment type
	     segments

	□Character type
	     characters *     lines

	□Graphic type
	     dots*     dots

	LCD Specification

	LCD type 
	□TN  □HTN  □STN  □FSTN  □TFT

	Image
	□Positive  □Negative

	Background Color
	□Gray  □Yellow green  □White(FSTN)  □Navy blue  □Black(FSTN)

	Polarizer
	□Reflective  □Transflective  □Transmissive  

	View direction
	□6:00  □12:00  □3:00  □9:00

	Printing
	□None  □Included

	Other 
	□Anti-UV  □Anti-glare

	Backlight 

	Backlight type
	□None  □LED-Array  □LED-Edge  □EL  □CCFL

	Color 
	□Amber  □Blue  □Orange  □Green  □Yellow green  □Red  □White  

	Built-in Inverter
	□None  □DC-AC  □DC-DC

	Temperature

	Operating
	        ~          ℃

	Storage
	        ~          ℃

	IC driver

	Controller
	□None  □         

	Booster
	□Negative Voltage Converter  □Positive Voltage Converter

	Fonts
	         


	Electrical characteristics

	Power supply
	VDD=          V, Idd=          mA

	Backlight 
	VLED=         V, If=          mA

	LCD driving
	VLCD=         V

	Connector

	□None (through hole)  □Connector           

	Frame

	□None  □Metal  □Plastic  □Others

	Special Request

	

	Remarks
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